Date and Time : 05/31/22 19:32:53

--------------------------------------------------
Checking Schematic: SCHEMATIC1
--------------------------------------------------
Checking Electrical Rules 
ERROR(ORCAP-1628): Possible pin type conflict +5V  Bidirectional Port Connected to Power
                    SCHEMATIC1, PAGE1  (124.46, 35.56) 
ERROR(ORCAP-1628): Possible pin type conflict +5V  Bidirectional Port Connected to Power
                    SCHEMATIC1, PAGE1  (35.56, 25.40) 
ERROR(ORCAP-1628): Possible pin type conflict +5V  Bidirectional Port Connected to Power
                    SCHEMATIC1, PAGE1  (68.58, 33.02) 
ERROR(ORCAP-1628): Possible pin type conflict U1,VCC  Power Connected to Bidirectional Port
                    SCHEMATIC1, PAGE1  (68.58, 40.64) 
ERROR(ORCAP-1628): Possible pin type conflict U2,V+  Power Connected to Bidirectional Port
                    SCHEMATIC1, PAGE1  (124.46, 40.64) 

Checking For Single Node Nets

Checking For Unconnected Bus Nets

Checking Physical Rules 


Checking Pins and Pin Connections

--------------------------------------------------
Checking Schematic: SCHEMATIC1
--------------------------------------------------

INFO(ORCAP-2242): Checking Incorrect Pin Group Assignment

Report for Invalid References

Report for Duplicate References

--------------------------------------------------
Checking Entire Design: LVDS DIFFERENTIAL SIGNALING DEMO 
--------------------------------------------------

Checking Power Pin Visibility  

Checking Normal Convert View Sync  
INFO(ORCAP-36105): Checking Missing Pin Numbers  

Checking Device with Zero pins  
INFO(ORCAP-36101): Checking Missing PCB Footprint Property  
#1 ERROR(ORCAP-36002): Property "PCB Footprint" missing from instance U2: SCHEMATIC1, PAGE1 (116.84, 40.64).

Checking Name Property for Hierarchical Instances  

INFO(ORCAP-2211): Check High Speed Properties Syntax

INFO(ORCAP-2212): Check Power Ground Mismatch
WARNING(ORCAP-1589): Net has two or more aliases that might lead to a short. Ensure nets are not shorted together or nets do not have two or more aliases. This message is displayed because 'Report all net names' is set in Design Rules Check dialog. U1,GND  GND  0
                    SCHEMATIC1, PAGE1  (68.58, 55.88) 
WARNING(ORCAP-1589): Net has two or more aliases that might lead to a short. Ensure nets are not shorted together or nets do not have two or more aliases. This message is displayed because 'Report all net names' is set in Design Rules Check dialog. U2,V-  V-  0
                    SCHEMATIC1, PAGE1  (124.46, 55.88) 

Reporting Unused Refdes in multiple part packages
Part	                       Quantity	                       Reference
-----------------------------------------------------------------------------------------
   SN55158_0	                       1	                       U1: B  
