# Static Call Graph for image .\Objects\STM32F4_DISCO_BSP.axf

#<CALLGRAPH># ARM Linker, 5060061: Last Updated: Wed Feb 28 19:23:30 2018

### Maximum Stack Usage = 248 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ drawaxes ⇒ ST7735_Drawaxes ⇒ ST7735_DrawChar ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - BusFault_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DebugMon_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - FPU_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - HardFault_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - MemManage_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - NMI_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PendSV_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - Reset_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SVC_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SysTick_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f411xe.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM2_IRQHandler from stm32f4_rtos_bsp.o(i.TIM2_IRQHandler) referenced from startup_stm32f411xe.o(RESET)
  - TIM3_IRQHandler from stm32f4_rtos_bsp.o(i.TIM3_IRQHandler) referenced from startup_stm32f411xe.o(RESET)
  - TIM4_IRQHandler from stm32f4_rtos_bsp.o(i.TIM4_IRQHandler) referenced from startup_stm32f411xe.o(RESET)
  - TIM5_IRQHandler from stm32f4_rtos_bsp.o(i.TIM5_IRQHandler) referenced from startup_stm32f411xe.o(RESET)
  - USART1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - UsageFault_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f411xe.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ drawaxes ⇒ ST7735_Drawaxes ⇒ ST7735_DrawChar ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f411xe.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ADC1_Init (Thumb, 144 bytes, Stack size 24 bytes, stm32f4_rtos_bsp.o(i.ADC1_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = ADC1_Init ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_ADC_Init
  - >> HAL_ADC_ConfigChannel
  [Called By]
  - >> main

  HAL_ADC_ConfigChannel (Thumb, 390 bytes, Stack size 12 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_ConfigChannel))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_ADC_ConfigChannel
  [Called By]
  - >> ADC1_Init

  HAL_ADC_GetValue (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_GetValue))
  [Called By]

  - >> main

  HAL_ADC_Init (Thumb, 100 bytes, Stack size 16 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> ADC_Init
  - >> HAL_ADC_MspInit
  [Called By]
  - >> ADC1_Init

  HAL_ADC_MspInit (Thumb, 70 bytes, Stack size 32 bytes, stm32f4_rtos_bsp.o(i.HAL_ADC_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_ADC_Init

  HAL_ADC_PollForConversion (Thumb, 186 bytes, Stack size 16 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_PollForConversion))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_ADC_PollForConversion
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> main

  HAL_ADC_Start (Thumb, 238 bytes, Stack size 8 bytes, stm32f4xx_hal_adc.o(i.HAL_ADC_Start))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_ADC_Start
  [Called By]
  - >> main

  HAL_Delay (Thumb, 26 bytes, Stack size 16 bytes, stm32f4xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> standard_Init_Cmd

  HAL_GPIO_Init (Thumb, 436 bytes, Stack size 24 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> ST7735_GPIO_Init
  - >> HAL_SPI_MspInit
  - >> Probe_Init
  - >> HAL_ADC_MspInit

  HAL_GPIO_TogglePin (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Called By]

  - >> Probe_CH0

  HAL_GPIO_WritePin (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> standard_Init_Cmd
  - >> lcd7735_sendData
  - >> lcd7735_sendCmd
  - >> writedata
  - >> writecommand
  - >> Probe_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_SPI_Transmit
  - >> HAL_Delay
  - >> HAL_ADC_PollForConversion
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> SPI_WaitFlagStateUntilTimeout

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> TIM2_IRQHandler

  HAL_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ TIM2_Init_Start ⇒ TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_MspInit
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 12 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 120
  - Call Chain = HAL_InitTick ⇒ TIM2_Init_Start ⇒ TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> TIM2_Init_Start
  [Called By]
  - >> HAL_Init
  - >> HAL_RCC_ClockConfig

  HAL_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal.o(i.HAL_MspInit))
  [Called By]

  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_TIM_Base_MspInit

  HAL_NVIC_SetPriority (Thumb, 124 bytes, Stack size 40 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> HAL_TIM_Base_MspInit

  HAL_NVIC_SetPriorityGrouping (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_RCC_ClockConfig (Thumb, 446 bytes, Stack size 16 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 136
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ TIM2_Init_Start ⇒ TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config80Mhz

  HAL_RCC_GetSysClockFreq (Thumb, 168 bytes, Stack size 16 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 1090 bytes, Stack size 16 bytes, stm32f4xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config80Mhz

  HAL_SPI_Init (Thumb, 160 bytes, Stack size 8 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> ST7735_SPI_Init

  HAL_SPI_MspInit (Thumb, 72 bytes, Stack size 32 bytes, glcd_st7735.o(i.HAL_SPI_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_SPI_Init

  HAL_SPI_Transmit (Thumb, 480 bytes, Stack size 32 bytes, stm32f4xx_hal_spi.o(i.HAL_SPI_Transmit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> SPI_WaitFlagStateUntilTimeout
  - >> SPI_CheckFlag_BSY
  [Called By]
  - >> lcd7735_senddata

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutationCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 98 bytes, Stack size 0 bytes, stm32f4xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Called By]

  - >> TIM2_Init

  HAL_TIM_Base_Init (Thumb, 52 bytes, Stack size 8 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> TIM2_Init

  HAL_TIM_Base_MspInit (Thumb, 236 bytes, Stack size 16 bytes, stm32f4_rtos_bsp.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> TIM2_Init_Start

  HAL_TIM_ConfigClockSource (Thumb, 306 bytes, Stack size 24 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> TIM2_Init

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 406 bytes, Stack size 8 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  - >> HAL_TIMEx_CommutationCallback
  - >> HAL_TIMEx_BreakCallback
  [Called By]
  - >> TIM5_IRQHandler
  - >> TIM4_IRQHandler
  - >> TIM3_IRQHandler
  - >> TIM2_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_PeriodElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  Probe_CH0 (Thumb, 12 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.Probe_CH0))
  [Stack]

  - Max Depth = 8
  - Call Chain = Probe_CH0
  [Calls]
  - >> HAL_GPIO_TogglePin
  [Called By]
  - >> main

  Probe_Init (Thumb, 68 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.Probe_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = Probe_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  ST7735_DrawChar (Thumb, 260 bytes, Stack size 56 bytes, glcd_st7735.o(i.ST7735_DrawChar))
  [Stack]

  - Max Depth = 176
  - Call Chain = ST7735_DrawChar ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> setAddrWindow
  - >> pushColor
  [Called By]
  - >> ST7735_Drawaxes

  ST7735_DrawCharS (Thumb, 236 bytes, Stack size 48 bytes, glcd_st7735.o(i.ST7735_DrawCharS))
  [Stack]

  - Max Depth = 200
  - Call Chain = ST7735_DrawCharS ⇒ ST7735_FillRect ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_FillRect
  - >> ST7735_DrawPixel
  [Called By]
  - >> ST7735_DrawString

  ST7735_DrawFastHLine (Thumb, 116 bytes, Stack size 32 bytes, glcd_st7735.o(i.ST7735_DrawFastHLine))
  [Stack]

  - Max Depth = 152
  - Call Chain = ST7735_DrawFastHLine ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> writedata
  - >> setAddrWindow
  [Called By]
  - >> ST7735_Drawaxes

  ST7735_DrawFastVLine (Thumb, 116 bytes, Stack size 32 bytes, glcd_st7735.o(i.ST7735_DrawFastVLine))
  [Stack]

  - Max Depth = 152
  - Call Chain = ST7735_DrawFastVLine ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> writedata
  - >> setAddrWindow
  [Called By]
  - >> ST7735_PlotIncrement
  - >> ST7735_Drawaxes

  ST7735_DrawPixel (Thumb, 64 bytes, Stack size 24 bytes, glcd_st7735.o(i.ST7735_DrawPixel))
  [Stack]

  - Max Depth = 144
  - Call Chain = ST7735_DrawPixel ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> setAddrWindow
  - >> pushColor
  [Called By]
  - >> ST7735_DrawCharS
  - >> ST7735_PlotPoint
  - >> ST7735_Drawaxes

  ST7735_DrawString (Thumb, 84 bytes, Stack size 32 bytes, glcd_st7735.o(i.ST7735_DrawString))
  [Stack]

  - Max Depth = 232
  - Call Chain = ST7735_DrawString ⇒ ST7735_DrawCharS ⇒ ST7735_FillRect ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_DrawCharS
  [Called By]
  - >> drawInfoBar

  ST7735_Drawaxes (Thumb, 270 bytes, Stack size 48 bytes, glcd_st7735.o(i.ST7735_Drawaxes))
  [Stack]

  - Max Depth = 224
  - Call Chain = ST7735_Drawaxes ⇒ ST7735_DrawChar ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_FillRect
  - >> ST7735_DrawPixel
  - >> ST7735_DrawFastVLine
  - >> ST7735_DrawFastHLine
  - >> ST7735_DrawChar
  [Called By]
  - >> drawaxes

  ST7735_FillRect (Thumb, 164 bytes, Stack size 32 bytes, glcd_st7735.o(i.ST7735_FillRect))
  [Stack]

  - Max Depth = 152
  - Call Chain = ST7735_FillRect ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> writedata
  - >> setAddrWindow
  [Called By]
  - >> ST7735_FillScreen
  - >> ST7735_DrawCharS
  - >> ST7735_Drawaxes

  ST7735_FillScreen (Thumb, 28 bytes, Stack size 16 bytes, glcd_st7735.o(i.ST7735_FillScreen))
  [Stack]

  - Max Depth = 168
  - Call Chain = ST7735_FillScreen ⇒ ST7735_FillRect ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_FillRect
  [Called By]
  - >> ST7735_Init

  ST7735_GPIO_Init (Thumb, 64 bytes, Stack size 32 bytes, glcd_st7735.o(i.ST7735_GPIO_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = ST7735_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> ST7735_Init

  ST7735_Init (Thumb, 40 bytes, Stack size 8 bytes, glcd_st7735.o(i.ST7735_Init))
  [Stack]

  - Max Depth = 176
  - Call Chain = ST7735_Init ⇒ ST7735_FillScreen ⇒ ST7735_FillRect ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> standard_Init_Cmd
  - >> ST7735_SetCursor
  - >> ST7735_SPI_Init
  - >> ST7735_GPIO_Init
  - >> ST7735_FillScreen
  [Called By]
  - >> main

  ST7735_PlotIncrement (Thumb, 46 bytes, Stack size 8 bytes, glcd_st7735.o(i.ST7735_PlotIncrement))
  [Stack]

  - Max Depth = 160
  - Call Chain = ST7735_PlotIncrement ⇒ ST7735_DrawFastVLine ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_DrawFastVLine
  [Called By]
  - >> plotData

  ST7735_PlotPoint (Thumb, 82 bytes, Stack size 16 bytes, glcd_st7735.o(i.ST7735_PlotPoint))
  [Stack]

  - Max Depth = 160
  - Call Chain = ST7735_PlotPoint ⇒ ST7735_DrawPixel ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_DrawPixel
  [Called By]
  - >> plotData

  ST7735_SPI_Init (Thumb, 56 bytes, Stack size 8 bytes, glcd_st7735.o(i.ST7735_SPI_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = ST7735_SPI_Init ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  [Called By]
  - >> ST7735_Init

  ST7735_SetCursor (Thumb, 22 bytes, Stack size 0 bytes, glcd_st7735.o(i.ST7735_SetCursor))
  [Called By]

  - >> ST7735_Init

  SystemClock_Config80Mhz (Thumb, 142 bytes, Stack size 80 bytes, stm32f4_rtos_bsp.o(i.SystemClock_Config80Mhz))
  [Stack]

  - Max Depth = 216
  - Call Chain = SystemClock_Config80Mhz ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ TIM2_Init_Start ⇒ TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  [Called By]
  - >> main

  SystemInit (Thumb, 82 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(.text)

  TIM2_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM2_IRQHandler ⇒ HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  TIM2_Init (Thumb, 70 bytes, Stack size 32 bytes, stm32f4_rtos_bsp.o(i.TIM2_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> TIM2_Init_Start

  TIM2_Init_Start (Thumb, 14 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.TIM2_Init_Start))
  [Stack]

  - Max Depth = 112
  - Call Chain = TIM2_Init_Start ⇒ TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority ⇒ __NVIC_SetPriority
  [Calls]
  - >> HAL_TIM_Base_Start_IT
  - >> TIM2_Init
  [Called By]
  - >> HAL_InitTick

  TIM3_IRQHandler (Thumb, 20 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.TIM3_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM3_IRQHandler ⇒ HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  TIM4_IRQHandler (Thumb, 20 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.TIM4_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM4_IRQHandler ⇒ HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  TIM5_IRQHandler (Thumb, 20 bytes, Stack size 8 bytes, stm32f4_rtos_bsp.o(i.TIM5_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM5_IRQHandler ⇒ HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  TIM_Base_SetConfig (Thumb, 148 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Called By]

  - >> HAL_TIM_Base_Init

  drawInfoBar (Thumb, 56 bytes, Stack size 8 bytes, main.o(i.drawInfoBar))
  [Stack]

  - Max Depth = 240
  - Call Chain = drawInfoBar ⇒ ST7735_DrawString ⇒ ST7735_DrawCharS ⇒ ST7735_FillRect ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_DrawString
  [Called By]
  - >> main

  drawaxes (Thumb, 44 bytes, Stack size 24 bytes, main.o(i.drawaxes))
  [Stack]

  - Max Depth = 248
  - Call Chain = drawaxes ⇒ ST7735_Drawaxes ⇒ ST7735_DrawChar ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_Drawaxes
  [Called By]
  - >> main

  lcd7735_sendCmd (Thumb, 24 bytes, Stack size 8 bytes, glcd_st7735.o(i.lcd7735_sendCmd))
  [Stack]

  - Max Depth = 96
  - Call Chain = lcd7735_sendCmd ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> lcd7735_senddata
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> standard_Init_Cmd

  lcd7735_sendData (Thumb, 22 bytes, Stack size 8 bytes, glcd_st7735.o(i.lcd7735_sendData))
  [Stack]

  - Max Depth = 96
  - Call Chain = lcd7735_sendData ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> lcd7735_senddata
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> standard_Init_Cmd

  lcd7735_senddata (Thumb, 16 bytes, Stack size 8 bytes, glcd_st7735.o(i.lcd7735_senddata))
  [Stack]

  - Max Depth = 88
  - Call Chain = lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_SPI_Transmit
  [Called By]
  - >> lcd7735_sendData
  - >> lcd7735_sendCmd
  - >> writedata
  - >> writecommand

  main (Thumb, 64 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 248
  - Call Chain = main ⇒ drawaxes ⇒ ST7735_Drawaxes ⇒ ST7735_DrawChar ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_Init
  - >> HAL_Init
  - >> HAL_ADC_Start
  - >> HAL_ADC_PollForConversion
  - >> HAL_ADC_GetValue
  - >> plotData
  - >> drawaxes
  - >> drawInfoBar
  - >> SystemClock_Config80Mhz
  - >> Probe_Init
  - >> Probe_CH0
  - >> ADC1_Init
  [Called By]
  - >> __rt_entry_main

  plotData (Thumb, 20 bytes, Stack size 8 bytes, main.o(i.plotData))
  [Stack]

  - Max Depth = 168
  - Call Chain = plotData ⇒ ST7735_PlotPoint ⇒ ST7735_DrawPixel ⇒ setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> ST7735_PlotPoint
  - >> ST7735_PlotIncrement
  [Called By]
  - >> main

  standard_Init_Cmd (Thumb, 92 bytes, Stack size 8 bytes, glcd_st7735.o(i.standard_Init_Cmd))
  [Stack]

  - Max Depth = 104
  - Call Chain = standard_Init_Cmd ⇒ lcd7735_sendData ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_Delay
  - >> lcd7735_sendData
  - >> lcd7735_sendCmd
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> ST7735_Init

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  pushColor (Thumb, 18 bytes, Stack size 8 bytes, glcd_st7735.o(i.pushColor))
  [Stack]

  - Max Depth = 104
  - Call Chain = pushColor ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> writedata
  [Called By]
  - >> ST7735_DrawPixel
  - >> ST7735_DrawChar

  setAddrWindow (Thumb, 106 bytes, Stack size 24 bytes, glcd_st7735.o(i.setAddrWindow))
  [Stack]

  - Max Depth = 120
  - Call Chain = setAddrWindow ⇒ writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> writedata
  - >> writecommand
  [Called By]
  - >> ST7735_FillRect
  - >> ST7735_DrawPixel
  - >> ST7735_DrawFastVLine
  - >> ST7735_DrawFastHLine
  - >> ST7735_DrawChar

  writecommand (Thumb, 24 bytes, Stack size 8 bytes, glcd_st7735.o(i.writecommand))
  [Stack]

  - Max Depth = 96
  - Call Chain = writecommand ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> lcd7735_senddata
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> setAddrWindow

  writedata (Thumb, 22 bytes, Stack size 8 bytes, glcd_st7735.o(i.writedata))
  [Stack]

  - Max Depth = 96
  - Call Chain = writedata ⇒ lcd7735_senddata ⇒ HAL_SPI_Transmit ⇒ SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> lcd7735_senddata
  - >> HAL_GPIO_WritePin
  [Called By]
  - >> ST7735_FillRect
  - >> ST7735_DrawFastVLine
  - >> ST7735_DrawFastHLine
  - >> setAddrWindow
  - >> pushColor

  ADC_Init (Thumb, 362 bytes, Stack size 0 bytes, stm32f4xx_hal_adc.o(i.ADC_Init))
  [Called By]

  - >> HAL_ADC_Init

  __NVIC_GetPriorityGrouping (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_hal_cortex.o(i.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> HAL_NVIC_SetPriority

  SPI_CheckFlag_BSY (Thumb, 40 bytes, Stack size 24 bytes, stm32f4xx_hal_spi.o(i.SPI_CheckFlag_BSY))
  [Stack]

  - Max Depth = 48
  - Call Chain = SPI_CheckFlag_BSY ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> HAL_SPI_Transmit

  SPI_WaitFlagStateUntilTimeout (Thumb, 170 bytes, Stack size 24 bytes, stm32f4xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_SPI_Transmit
  - >> SPI_CheckFlag_BSY

  TIM_ETR_SetConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f4xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_ITRx_SetConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_TI1_ConfigInputStage (Thumb, 42 bytes, Stack size 12 bytes, stm32f4xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 44 bytes, Stack size 12 bytes, stm32f4xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  ### Undefined Global Symbols