### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.
To see the actual file transmitted to Xilinx, please click here.

software_version_and_target_device
date_generated | Sat Apr 22 17:51:08 2017 | product_version | Vivado v2015.4 (64-bit)
build_version | 1412921 | os_platform | WIN64
registration_id | 211139803_0_0_561 | tool_flow | Vivado
beta | FALSE | route_design | TRUE
target_family | artix7 | target_device | xc7a35t
target_package | cpg236 | target_speed | -2
random_id | fa2d7df0d966501b95ccc4b479e89299 | project_id | b121af2fe6644b62b446fef50c90bef0
project_iteration | 1

user_environment
os_name | Microsoft Windows 7 , 64-bit | os_release | Service Pack 1 (build 7601)
cpu_name | Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz | cpu_speed | 1995 MHz
total_processors | 1 | system_ram | 6.000 GB

vivado_usage

project_data
srcsetcount=6 | constraintsetcount=1 | designmode=RTL | prproject=false
reconfigpartitioncount=0 | reconfigmodulecount=0 | hdproject=false | partitioncount=0
synthesisstrategy=Vivado Synthesis Defaults | implstrategy=Vivado Implementation Defaults | currentsynthesisrun=synth_1 | currentimplrun=impl_1
totalsynthesisruns=1 | totalimplruns=1 | core_container=false

other_data
guimode=1

unisim_transformation
pre_unisim_transformation
bufg=1 | carry4=27 | fdce=79 | fdre=342
fdse=21 | gnd=277 | ibuf=5 | lut1=31
lut2=49 | lut3=62 | lut4=229 | lut5=80
lut6=172 | lut6_2=79 | muxf7=32 | obuf=16
ram32x1d=64 | ramb36e1=16 | srl16e=46 | vcc=77
xadc=1
post_unisim_transformation
bufg=1 | carry4=27 | fdce=79 | fdre=342
fdse=21 | gnd=277 | ibuf=5 | lut1=31
lut2=49 | lut3=62 | lut4=229 | lut5=159
lut6=251 | muxf7=32 | obuf=16 | ramb36e1=16
ramd32=128 | srl16e=46 | vcc=77 | xadc=1

power_opt_design
usage
slice_registers_augmented=0 | slice_registers_newly_gated=0 | slice_registers_total=378 | srls_augmented=0
srls_newly_gated=0 | srls_total=46 | bram_ports_augmented=0 | bram_ports_newly_gated=0
bram_ports_total=32 | flow_state=default
command_line_options_spo
-clocks=default::[not_specified] | -include_cells=default::[not_specified] | -exclude_cells=default::[not_specified] | -cell_types=default::all

ip_statistics
Hex_to_7_Seg/1
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=Hex_to_7_Seg | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED
Hex_to_7_Seg/2
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=Hex_to_7_Seg | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED
Hex_to_7_Seg/3
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=Hex_to_7_Seg | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED
Hex_to_7_Seg/4
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=Hex_to_7_Seg | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED
Hex_to_7_Seg/5
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=Hex_to_7_Seg | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED
IP_Integrator/1
iptotal=1 | core_container=NA | x_ipvendor=xilinx.com | x_iplibrary=BlockDiagram
x_ipname=design_1 | x_ipversion=1.00.a | x_iplanguage=VHDL | numblks=12
numreposblks=12 | numnonxlnxblks=0 | numhierblks=0 | maxhierdepth=0
synth_mode=Global
Seg_Display_16/1
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=Seg_Display_16 | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED | input_clk_freq=100000000 | refresh_rate=50000
binary_bcd/1
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=user | x_ipname=binary_bcd | x_ipversion=1.0 | x_ipcorerevision=2
x_iplanguage=VHDL | x_ipsimlanguage=MIXED | n=16
microblaze_mcs/1
iptotal=1 | core_container=NA | x_ipproduct=Vivado 2015.4 | x_ipvendor=xilinx.com
x_iplibrary=ip | x_ipname=microblaze_mcs | x_ipversion=2.3 | x_ipcorerevision=3
x_iplanguage=VHDL | x_ipsimlanguage=MIXED | c_family=artix7 | c_microblaze_instance=design_1_microblaze_mcs_0_0
c_avoid_primitives=0 | c_path=mcs_0/U0 | c_freq=100000000 | c_memsize=65536
c_debug_enabled=0 | c_jtag_chain=2 | c_trace=0 | c_use_io_bus=0
c_use_uart_rx=0 | c_use_uart_tx=0 | c_uart_baudrate=9600 | c_uart_data_bits=8
c_uart_use_parity=0 | c_uart_odd_parity=0 | c_uart_rx_interrupt=0 | c_uart_tx_interrupt=0
c_uart_error_interrupt=0 | c_uart_prog_baudrate=0 | c_use_fit1=0 | c_fit1_no_clocks=6216
c_fit1_interrupt=0 | c_use_fit2=0 | c_fit2_no_clocks=6216 | c_fit2_interrupt=0
c_use_fit3=0 | c_fit3_no_clocks=6216 | c_fit3_interrupt=0 | c_use_fit4=0
c_fit4_no_clocks=6216 | c_fit4_interrupt=0 | c_use_pit1=0 | c_pit1_size=32
c_pit1_readable=1 | c_pit1_prescaler=0 | c_pit1_interrupt=0 | c_use_pit2=0
c_pit2_size=32 | c_pit2_readable=1 | c_pit2_prescaler=0 | c_pit2_interrupt=0
c_use_pit3=0 | c_pit3_size=32 | c_pit3_readable=1 | c_pit3_prescaler=0
c_pit3_interrupt=0 | c_use_pit4=0 | c_pit4_size=32 | c_pit4_readable=1
c_pit4_prescaler=0 | c_pit4_interrupt=0 | c_use_gpo1=1 | c_gpo1_size=7
c_gpo1_init=0x00000000 | c_use_gpo2=1 | c_gpo2_size=16 | c_gpo2_init=0x00000000
c_use_gpo3=1 | c_gpo3_size=7 | c_gpo3_init=0x00000000 | c_use_gpo4=0
c_gpo4_size=32 | c_gpo4_init=0x00000000 | c_use_gpi1=1 | c_gpi1_size=16
c_gpi1_interrupt=0 | c_use_gpi2=1 | c_gpi2_size=1 | c_gpi2_interrupt=0
c_use_gpi3=0 | c_gpi3_size=32 | c_gpi3_interrupt=0 | c_use_gpi4=0
c_gpi4_size=32 | c_gpi4_interrupt=0 | c_intc_use_ext_intr=0 | c_intc_intr_size=1
c_intc_level_edge=0x0000 | c_intc_positive=0xFFFF | c_intc_async_intr=0xFFFF | c_intc_num_sync_ff=2
xadc_wiz_v3_2_0/1
iptotal=1 | core_container=false | component_name=design_1_xadc_wiz_0_0 | enable_axi=false
enable_axi4stream=false | dclk_frequency=100 | enable_busy=true | enable_convst=false
enable_convstclk=false | enable_dclk=true | enable_drp=true | enable_eoc=true
enable_eos=true | enable_vbram_alaram=false | enable_vccddro_alaram=false | enable_vccint_alaram=false
enable_vccaux_alaram=falseenable_vccpaux_alaram=false | enable_vccpint_alaram=false | ot_alaram=false | user_temp_alaram=false
timing_mode=continuous | channel_averaging=None | sequencer_mode=off | startup_channel_selection=single_channel

report_utilization
slice_logic
slice_luts_used=732 | slice_luts_fixed=0 | slice_luts_available=20800 | slice_luts_util_percentage=3.52
lut_as_logic_used=564 | lut_as_logic_fixed=0 | lut_as_logic_available=20800 | lut_as_logic_util_percentage=2.71
lut_as_memory_used=168 | lut_as_memory_fixed=0 | lut_as_memory_available=9600 | lut_as_memory_util_percentage=1.75
lut_as_distributed_ram_used=128 | lut_as_distributed_ram_fixed=0 | lut_as_shift_register_used=40 | lut_as_shift_register_fixed=0
slice_registers_used=378 | slice_registers_fixed=0 | slice_registers_available=41600 | slice_registers_util_percentage=0.91
register_as_flip_flop_used=378 | register_as_flip_flop_fixed=0 | register_as_flip_flop_available=41600 | register_as_flip_flop_util_percentage=0.91
register_as_latch_used=0 | register_as_latch_fixed=0 | register_as_latch_available=41600 | register_as_latch_util_percentage=0.00
f7_muxes_used=32 | f7_muxes_fixed=0 | f7_muxes_available=16300 | f7_muxes_util_percentage=0.20
f8_muxes_used=0 | f8_muxes_fixed=0 | f8_muxes_available=8150 | f8_muxes_util_percentage=0.00
slice_used=243 | slice_fixed=0 | slice_available=8150 | slice_util_percentage=2.98
slicel_used=168 | slicel_fixed=0 | slicem_used=75 | slicem_fixed=0
lut_as_logic_used=564 | lut_as_logic_fixed=0 | lut_as_logic_available=20800 | lut_as_logic_util_percentage=2.71
using_o5_output_only_used=0 | using_o5_output_only_fixed= | using_o6_output_only_used=400 | using_o6_output_only_fixed=
using_o5_and_o6_used=164 | using_o5_and_o6_fixed= | lut_as_memory_used=168 | lut_as_memory_fixed=0
lut_as_memory_available=9600 | lut_as_memory_util_percentage=1.75 | lut_as_distributed_ram_used=128 | lut_as_distributed_ram_fixed=0
using_o5_output_only_used=0 | using_o5_output_only_fixed= | using_o6_output_only_used=128 | using_o6_output_only_fixed=
using_o5_and_o6_used=0 | using_o5_and_o6_fixed= | lut_as_shift_register_used=40 | lut_as_shift_register_fixed=0
using_o5_output_only_used=0 | using_o5_output_only_fixed= | using_o6_output_only_used=34 | using_o6_output_only_fixed=
using_o5_and_o6_used=6 | using_o5_and_o6_fixed= | lut_flip_flop_pairs_used=816 | lut_flip_flop_pairs_fixed=0
lut_flip_flop_pairs_available=20800 | lut_flip_flop_pairs_util_percentage=3.92 | fully_used_lut_ff_pairs_used=224 | fully_used_lut_ff_pairs_fixed=
lut_ff_pairs_with_unused_lut_used=84 | lut_ff_pairs_with_unused_lut_fixed= | lut_ff_pairs_with_unused_flip_flop_used=508 | lut_ff_pairs_with_unused_flip_flop_fixed=
unique_control_sets_used=27 | minimum_number_of_registers_lost_to_control_set_restriction_used=94(Lost)
memory
block_ram_tile_used=16 | block_ram_tile_fixed=0 | block_ram_tile_available=50 | block_ram_tile_util_percentage=32.00
ramb36_fifo_used=16 | ramb36_fifo_fixed=0 | ramb36_fifo_available=50 | ramb36_fifo_util_percentage=32.00
ramb36e1_only_used=16 | ramb18_used=0 | ramb18_fixed=0 | ramb18_available=100
ramb18_util_percentage=0.00
dsp
dsps_used=0 | dsps_fixed=0 | dsps_available=90 | dsps_util_percentage=0.00
clocking
bufgctrl_used=1 | bufgctrl_fixed=0 | bufgctrl_available=32 | bufgctrl_util_percentage=3.13
bufio_used=0 | bufio_fixed=0 | bufio_available=20 | bufio_util_percentage=0.00
mmcme2_adv_used=0 | mmcme2_adv_fixed=0 | mmcme2_adv_available=5 | mmcme2_adv_util_percentage=0.00
plle2_adv_used=0 | plle2_adv_fixed=0 | plle2_adv_available=5 | plle2_adv_util_percentage=0.00
bufmrce_used=0 | bufmrce_fixed=0 | bufmrce_available=10 | bufmrce_util_percentage=0.00
bufhce_used=0 | bufhce_fixed=0 | bufhce_available=72 | bufhce_util_percentage=0.00
bufr_used=0 | bufr_fixed=0 | bufr_available=20 | bufr_util_percentage=0.00
specific_feature
bscane2_used=0 | bscane2_fixed=0 | bscane2_available=4 | bscane2_util_percentage=0.00
capturee2_used=0 | capturee2_fixed=0 | capturee2_available=1 | capturee2_util_percentage=0.00
dna_port_used=0 | dna_port_fixed=0 | dna_port_available=1 | dna_port_util_percentage=0.00
efuse_usr_used=0 | efuse_usr_fixed=0 | efuse_usr_available=1 | efuse_usr_util_percentage=0.00
frame_ecce2_used=0 | frame_ecce2_fixed=0 | frame_ecce2_available=1 | frame_ecce2_util_percentage=0.00
icape2_used=0 | icape2_fixed=0 | icape2_available=2 | icape2_util_percentage=0.00
pcie_2_1_used=0 | pcie_2_1_fixed=0 | pcie_2_1_available=1 | pcie_2_1_util_percentage=0.00
startupe2_used=0 | startupe2_fixed=0 | startupe2_available=1 | startupe2_util_percentage=0.00
xadc_used=1 | xadc_fixed=1 | xadc_available=1 | xadc_util_percentage=100.00
primitives
fdre_used=294 | fdre_functional_category=Flop & Latch | lut6_used=193 | lut6_functional_category=LUT
lut5_used=181 | lut5_functional_category=LUT | lut4_used=164 | lut4_functional_category=LUT
ramd32_used=128 | ramd32_functional_category=Distributed Memory | lut3_used=102 | lut3_functional_category=LUT
lut2_used=83 | lut2_functional_category=LUT | fdce_used=63 | fdce_functional_category=Flop & Latch
srl16e_used=46 | srl16e_functional_category=Distributed Memory | muxf7_used=32 | muxf7_functional_category=MuxFx
carry4_used=27 | carry4_functional_category=CarryLogic | fdse_used=21 | fdse_functional_category=Flop & Latch
ramb36e1_used=16 | ramb36e1_functional_category=Block Memory | obuf_used=16 | obuf_functional_category=IO
lut1_used=5 | lut1_functional_category=LUT | ibuf_used=5 | ibuf_functional_category=IO
xadc_used=1 | xadc_functional_category=Others | bufg_used=1 | bufg_functional_category=Clock
io_standard
diff_sstl15_r=0 | hstl_ii=0 | lvcmos15=0 | blvds_25=0
lvttl=0 | diff_sstl15=0 | hstl_i=0 | lvcmos25=0
diff_mobile_ddr=0 | lvcmos33=1 | pci33_3=0 | hsul_12=0
lvcmos18=0 | mobile_ddr=0 | lvcmos12=0 | diff_hsul_12=0
hstl_i_18=0 | hstl_ii_18=0 | sstl18_i=0 | sstl18_ii=0
sstl15=0 | sstl15_r=0 | sstl135=0 | sstl135_r=0
lvds_25=0 | diff_hstl_i=0 | rsds_25=0 | diff_hstl_ii=0
tmds_33=0 | diff_hstl_i_18=0 | mini_lvds_25=0 | diff_hstl_ii_18=0
ppds_25=0 | diff_sstl18_i=0 | diff_sstl18_ii=0 | diff_sstl135=0
diff_sstl135_r=0

router
usage
lut=748 | ff=378 | bram36=16 | bram18=0
ctrls=27 | dsp=0 | iob=21 | bufg=0
global_clocks=1 | pll=0 | bufr=0 | nets=1831
movable_instances=1644 | pins=12571 | bogomips=0 | high_fanout_nets=2
effort=2 | threads=2 | router_timing_driven=1 | timing_constraints_exist=1
estimated_expansions=1603950 | actual_expansions=1614001 | router_runtime=32.677000

synthesis
command_line_options
-part=xc7a35tcpg236-2 | -name=default::[not_specified] | -top=design_1_wrapper | -include_dirs=default::[not_specified]
-generic=default::[not_specified] | -verilog_define=default::[not_specified] | -constrset=default::[not_specified] | -seu_protect=default::none
-flatten_hierarchy=default::rebuilt | -gated_clock_conversion=default::off | -directive=default::default | -rtl=default::[not_specified]
-link_dcps=default::[not_specified] | -rtl_load_constraints=default::[not_specified] | -bufg=default::12 | -fanout_limit=default::10000
-shreg_min_size=default::3 | -mode=default::default | -fsm_extraction=default::auto | -keep_equivalent_registers=default::[not_specified]
-resource_sharing=default::auto | -cascade_dsp=default::auto | -control_set_opt_threshold=default::auto
usage
elapsed=00:01:07s | memory_peak=666.688MB | memory_gain=453.078MB | hls_ip=0